CMOS Info:

Used 3- decoders for addressing the memory

A0 acts as BLE

BHE from microprocessor

Need to connect the write and read pins and input/ouput stuff

Address range is 00000H-FFFFFH